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INSTRUCTION SHEET

     As shown in diagram above, place the Foam Precleaner(1) in Filter Housing(2) and then place the Filter(3) on top of the Foam Precleaner(1).  Sealing surface of Filter(4) should be located at the rim of the Filter Housing after insertion.  At this point, the Filter Housing top can be put in place and tightened down for proper installation.  

FEUILLE D(INSTRUCTION
Comme le montre le schéma ci-dessus, placez le préfiltre en mousse (1) dans le boîtier du filtre (2), puis placez le filtre (3) au-dessus du préfiltre en mousse (1).  La surface d(étanchéité du filtre (4) doit être placée au bord du boîtier du filtre après insertion.  À ce point, la partie supérieure du boîtier du filtre peut être mise en place et serrée pour achever l(installation.

HOJA DE INSTRUCCIONES
Tal como se muestra en el diagrama de arriba, coloque el pre-filtrador de espuma (1) dentro de la caja protectora del filtro (2), y luego coloque el filtro (3) encima de dicho pre-filtrador de espuma (1). La superficie de sellado del filtro (4) debe quedar ubicada en el borde de la caja protectora del filtro, luego de la inserción. En este momento, la parte superior de la caja protectora del filtro puede ser colocada en su lugar y ajustada hacia abajo, para una instalación correcta.
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