Cabin Air Installation Instructions

Hyundai , Kia Instructions

Estimated installation time (minutes): 10

The cabin air filter is located behind the glove-box and the glove-box must be removed.

1.  •   Open glove-box.

2.  •
  Press in on both sides of the glove-box to clear the stops and lower the glove- box downward.

3.  •   This exposes the cabin air cover – release the tabs – remove the old filter and replace.
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 Mode d’installation du filtre d’habitacle

Directives pour Hyundai et Kia

Durée d’installation estimée (en minutes) : 10

Le filtre d’habitacle est situé derrière la boîte à gants, qui doit être déposée.

1.  •
 Ouvrez la boîte à gants.

2.  •
 Appuyez sur les deux côtés de la boîte à gants pour dégager les pattes, puis déplacez la boîte à gants vers le bas.

3.  •
 Ceci expose le couvercle du filtre d’habitacle; dégagez les pattes; retirez le filtre usé et remplacez-le.
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 Instrucciones para la instalación del filtro de aire de la cabina

Instrucciones para vehículos Hyundai y Kia

Duración estimada de la instalación (en minutos): 10

El filtro de aire de la cabina está situado detrás de la guantera y la misma debe ser quitada.

1. •
Abra la guantera.

2. •
Presione sobre ambos lados de la guantera para liberar los topes y poder desplazar la guantera hacia abajo.

3. •
Esto deja expuesta a la cubierta del filtro de aire de la cabina. Libere las lengüetas, quite el filtro viejo y 

        reemplácelo.
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